For 1990-2009 cars

Condition | Possible Cause
--- | ---
Fluid pressure High or Low |

• | Fluid pump internal leak

• | Fluid pump drive and driven gears worn or damaged

• | Fluid pump cover seal rings cut or damaged

• | Fluid pump body or cover casting porous or damaged

• | TV cable link loose or disconnected

• | TV cable out of adjustment, binding or damaged

• | Valve body spacer plate or gaskets improper position or damaged

• | Check balls omitted or improper position

• | Manual valve binding or sticking

• | Manual valve link disconnected

• | Primary regulator valve binding or sticking

• | Case internal leak in forward clutch fluid circuit

• | Case internal leak in direct clutch fluid circuit

• | Case fluid passages blocked or restricted