For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Disconnect the vehicle speed sensor connector (1).
3. Remove the 1 retaining bolt (3) and the VSS from the transaxle.
4. Inspect the VSS O-ring for damage. Replace the O-ring, as necessary.

### Installation Procedure

1. Install the O-ring onto the vehicle speed sensor (VSS) (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the VSS (4) into the transaxle case. Secure the VSS with the retaining bolt (3).

Tighten
Tighten the VSS retaining bolt (3) to 23 N·m (17 lb ft).

3. Connect the VSS electrical connector (1) .
4. Connect the negative battery cable.