For 1990-2009 cars

### Removal Procedure

1. Open the liftgate.
2. Lower the rear seat.
3. Fold back the carpet and the spare tire cover in order to gain access to the trim panel plastic retaining clips.
4. Remove the following components that secure the quarter panel inner front trim (2) to the vehicle:

• | The 4 screws

• | The plastic retaining clip

5. Unclip the bottom of the rear seat in order to gain access to the rear side sill scuff panel (9).
6. Unclip the front side sill scuff panel (11) from the rear side scuff panel (9).
7. Remove the 4 plastic retaining clips that secure the rear side scuff panel.
8. Remove the rear side scuff panel from the vehicle.
9. Unclip and remove the quarter panel inner front trim (2) from the vehicle.

### Installation Procedure

1. Position the quarter panel inner front trim (2) into the vehicle. Snap the trim into place.
2. Install the rear side scuff panel. Secure the scuff panel (9) with 4 plastic retaining clips.
3. Clip the front side sill scuff panel (11) into the rear side scuff panel (9). Secure the panel with the plastic retaining clip.
4. Reposition the bottom of the rear seat back into place.
5. Install the following components in order to secure the front trim (2) of the quarter panel liner to the vehicle:

• | The 4 screws

• | The plastic retaining clip

6. Reposition the carpet and the spare tire cover.
7. Reposition the rear seat.
8. Close the liftgate.