For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Open the rear compartment lid.
3. Using a flat-bladed tool, gently remove the plastic lamp cover (3).
4. Remove the bulb (2) from the socket (1).

### Installation Procedure

1. Install the bulb (2) to the socket (1).
2. Install the plastic lamp cover (3).
3. Close the rear compartment lid.
4. Connect the negative battery cable.