For 1990-2009 cars

# REVISED: KEY CODING IDENTIFICATION

KEY CODING INFORMATION - 1985-86 SPRINT, FIREFLY, SPECTRUM, SUNBURST, AND NOVA MODELS

#### VEHICLES AFFECTED: 1985-86 Sprint, Firefly Spectrum, Sunburst ----------------- and Nova Models

This information is intended to assist Service Technicians in properly identifying key codes, and suggested equipment for cutting new keys when required. This also updates Product Service Bulletin 85-2-143 dated July 8/85.

#### KEY CODING (1985-86 SPECTRUM AND SUNBURST)

#### Key Usage Identification

One key is used for the ignition, door, instrument panel compartment and trunk lock cylinders. The keys are cut on both edges to make them reversible. Key identification is obtained from the five character key code stamped on the key code tag. From this key code, the key code cutting combination can be determined from a code list supplied by GM Parts, Curtis Industries, or available to owners of key cutting equipment from suppliers.

KEY CODING (1985-86 NOVA)

#### Key Usage and Identification

Two keys are used, one key is used for the ignition, while the other is for the door, instrument panel compartment and trunk lock cylinders. Both keys are cut on both sides to make them reversible.

Key identification is obtained from the four character key code stamped on the key code tag. From this key code, the key code cutting combination can be determined from a code list supplied by GM Parts, Curtis Industries, or available to owners of key cutting equipment from suppliers.

KEY CODE LOCATION (1985-86 SPRINT, FIREFLY, SPECTRUM, SUNBURST, & NOVA -----------------------------------------------------

If key codes are not available from records or tags, the key code can be obtained from the right hand door lock cylinder (if lock has not been replaced). Lock cylinders supplied by the factory as service parts are unmarked.

If the original key is available, the key code cutting combination can be determined by laying the key on the diagram shown in the Shop Manual for the designated model.

#### KEY TYPES (1985-86) SPECTRUM AND SUNBURST ONLY

The key comes in Types A or B, depending on the key code combination. When the first position in the combination is a 1, 2 or 3, Style A is used. When the first position in the combination is a 4, Style B (factory pre-cut key) is used.

#### KEY TYPES (1985-86 NOVA ONLY)

The ignition key, stamped 'R', can only be ordered with a plastic protector.

The door, trunk etc., key, stamped 'S', can only be ordered without a plastic protector. Model Sprint/Firefly Spectrum/Sunburst Nova ----- -------------- ----------------- ----

No. of Keys 1 1 2 Per Vehicle

Ignition 96052124 94148551 (Type A) 94843836 GM Part No. 94148552 (Type B)

Door, Trunk, Etc. Same as ignition Same as ignition 94843835 GM Part No.

* Curtis Code Cutter No. 15 15 15

* Curtis Carriage No. DC-1 Toy-7B Toy-4('R') Toy-4('S') * Curtis Cam-Set No. DC-1 15N-6 DC-1

Parts & Accessories Key Code 85-45 85-45 35-110 Bulletin No. (GM Parts) March 8, 1985 March 8, 1985 June 12, 1985 * Or Equivalent

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.