For 1990-2009 cars

### Removal Procedure

1. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Release the 4 tabs that retain the inner sealing strip (3) to the door trim (4).

### Installation Procedure

1. Insert the tabs of the inner sealing strip (3) into the door trim (4). Fold the tabs over.
2. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .