For 1990-2009 cars

1. Remove the intermediate band anchor pin (750).

Important: While performing the next step, be careful not to drop the front planetary ring gear bearing or the races, which may adhere to the forward clutch assembly.

2. Remove the direct clutch (793) and the forward clutch (781) assemblies by grasping the input shaft (776) in your hand and gently lift up.
3. Remove the intermediate band (751) from the transaxle case.
4. Remove the direct clutch assembly (793) from the forward clutch housing (781) and the input shaft (776).
5. Remove the intermediate band from the transaxle case.