For 1990-2009 cars

Inspect the following components:

• | The joints from the column to the steering gear for wear

• | The joints from the column to the steering gear for improper installation

• | The steering gear valve for proper installation

• | The power steering pump for the sufficient pressure output

• | The power steering pump for internal leakage

• | The steering gear for internal leakage

• | The steering hydraulic system

• | The steering gear for binding and rough movement

• | The steering gear mounting for proper and secure installation

• | The tires for adequate inflation