For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
2nd Brake Solenoid Retaining Bolt | 4 N·m | 35 lb in
Ball Stud Nuts and Bolts | 60 N·m | 44 lb ft
Direct Clutch Solenoid Retaining Bolt | 4 N·m | 35 lb in
Engine Wiring Harness Bracket Bolts | 16 N·m | 12 lb ft
Filler Tube Bracket Bolt | 6 N·m | 53 lb in
Fluid Filter Screen Bolts | 6 N·m | 53 lb in
Flywheel Cover Bolts | 10 N·m | 89 lb in
Flywheel-to-Torque Converter Bolts | 19 N·m | 14 lb ft
Inlet and Outlet Union Bolts | 22 N·m | 16 lb ft
Interlock Cable Bolt | 13 N·m | 115 lb in
Left Transaxle Mount Bracket Bolts | 55 N·m | 40 lb ft
Left Transaxle Mount Retaining Nuts | 55 N·m | 40 lb ft
Line PressureTap Bolt | 9 N·m | 80 lb in
Lower Engine-to-Transaxle Retaining Bolt and Nut | 55 N·m | 40 lb ft
Lower Rear Engine Mount-to-Bulkhead Bolt | 55 N·m | 40 lb ft
Lower Valve Body Bolts | 12 N·m | 106 lb in
Lower Valve Body Cover Bolts | 4 N·m | 35 lb in
Negative (-) Battery Cable-to-Transaxle Case Bolt | 15 N·m | 11 lb ft
Park/Neutral Position Switch Mounting Bolt | 23 N·m | 17 lb ft
Rear Engine Mount Bracket Bolts and Nuts | 55 N·m | 40 lb ft
Rear Engine Torque Rod Assembly Bolts | 55 N·m | 40 lb ft
Selector Lever Assembly Housing Seat Nuts | 16 N·m | 11.5 lb ft
Shift Select Cable Bulkhead Grommet Bolts | 20 N·m | 15 lb ft
Solenoid Wiring Harness Retaining Bracket Bolt | 20 N·m | 15 lb ft
Solenoid Wiring Harness Retaining Plate Nut | 20 N·m | 15 lb ft
Speedometer Driven Gear Case Retaining Bolt | 8 N·m | 11 lb ft
Starter Motor Retaining Bolts | 23 N·m | 17 lb ft
Transaxle Cooler Pipe Retaining Bracket Bolt | 10 N·m | 7.5 lb in
Transaxle Drain Plug | 23 N·m | 17 lb ft
Transaxle Fluid Pan Bolts | 6 N·m | 53 lb in
Upper Rear Transaxle Mount-to-Bulkhead Bolt | 55 N·m | 40 lb ft
Upper Transaxle-to-Engine Retaining Bolts | 55 N·m | 40 lb ft
Upper Valve Body Bolts | 6 N·m | 53 lb in
Vehicle Speed Sensor (VSS) Retaining Bolt | 23 N·m | 17 lb ft