For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Automatic Transaxle Ground Bolt | 50 N·m | 37 lb ft
Battery Cable-to-Battery Terminals | 5.5 N·m | 48.68 lb in
Battery Cable-to-Battery Terminal Retainers | 15 N·m | 11 lb ft
Battery Retainer Bracket Bolts | 8 N·m | 71 lb in
Battery Terminal Retaining Nut | 10 N·m | 89 lb in
Body Ground Bolt | 8 N·m | 71 lb in
Camshaft Position (CMP) Sensor Retaining Screws | 5 N·m | 44 lb in
Commutator End Cover Bolts | 8 N·m | 71 lb in
Distributor Flange Bolts | 15 N·m | 11 lb ft
Drive Pulley Retaining Nut | 65 N·m | 48 lb ft
Field Coil Lead Wire Retaining Nut | 10 N·m | 89 lb in
Frame Bolts and Nuts | 30 N·m | 22 lb ft
Generator B Terminal Nut | 10 N·m | 89 lb in
Generator Housing Bolts | 30 N·m | 22 lb ft
Generator Mounting Bolts | 23 N·m | 17 lb ft
Ignition Coil Mounting Bracket Bolts | 15 N·m | 11 lb ft
Manual Transaxle Ground Bolt | 23 N·m | 17 lb ft
Positive Battery Cable-to-Solenoid Retaining Nut | 10 N·m | 89 lb in
Solenoid Mounting Nuts | 7 N·m | 62 lb in
Spark Plugs | 28 N·m | 21 lb ft
Starter Motor Assembly Mounting Bolts | 23 N·m | 17 lb ft
Stator Stud Bolts | 8 N·m | 71 lb in