For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the hood.
2. Mark the position of the bolts to the hood latch (1).
3. Remove the following components from the vehicle:

3.1. | the 3 bolts

3.2. | The hood latch (1)

4. Remove the hood latch release cable (2) from the hood latch (1).

### Installation Procedure

1. Install the hood latch release cable (2) to the hood latch (1). Secure the latch with 4 bolts. Do NOT completely tighten the bolts.
2. Align the striker shaft with the center groove of the hood latch.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Align the hood latch (1) with the front fender. Refer to Body Front End Adjustment Specifications .

Tighten
Tighten the hood latch bolts to 7 N·m (62 lb in).

4. Lower the hood.