For 1990-2009 cars

The service procedures contained in this section are common to the Suzuki 3-speed automatic transaxle.

For complete transaxle unit repair procedures, refer to the Transmission Unit Repair Manual.

#### Clutch Application

Range | Gear | Forward Clutch (5) | Direct Clutch (4) | 2nd Brake Band | 1st and Reverse Brake | One-Way Clutch | Parking Lock Pawl
--- | --- | --- | --- | --- | --- | --- | ---
P | Parking | -- | -- | -- | **X | -- | X
R | Reverse | -- | X | -- | X | -- | --
N | Neutral | -- | -- | -- | -- | -- | --
D | 1st | X | -- | -- | -- | X | --
2nd | X | -- | X | -- | -- | --
3rd | X | X | -- | -- | -- | --
2 | 1st | X | -- | -- | -- | X | --
2nd | X | -- | X | -- | -- | --
1 | 1st | X | -- | -- | X | X | --
**2nd | X | -- | X | -- | -- | --
X = Applied * = In order to prevent overrevolution of the engine, this 2nd gear is operated only when the selector lever is shifted to L range at the speed of more than 55 km/h (34 mph) ** = When engine is running