For 1990-2009 cars

### Removal Procedure

1. Raise the rear compartment lid (10).
2. Fold back the carpet and spare tire cover in order to gain access to the rear end interior trim panel plastic retaining clips.
3. Remove the following components from the vehicle:

• | 9 clips

• | The rear end interior trim panel (5)

4. Remove the cover of the lock striker (6) .
5. Disconnect the lamp switch electrical connector.
6. Remove the following components from the lock striker (6):

• | 1 screw

• | The lamp switch

### Installation Procedure

1. Install the lamp switch to the lock striker (6). Secure the switch with 1 screw.
2. Connect the lamp switch electrical connector.
3. Install the cover of the lock striker (6).
4. Install the rear end interior trim panel (5). Secure the panel with 9 clips.
5. Reposition the rear compartment carpet back to it's original position.
6. Lower the rear compartment lid (10).