For 1990-2009 cars

### Removal Procedure

1. Discharge and recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Disconnect the pipe fitting at the condenser outlet.
3. Remove the bolt and the receiver/dryer inlet pipe (4) from the receiver/dryer.

### Installation Procedure

1. Coat new O-rings with mineral base 525 viscosity refrigerant oil.
2. Install the O-rings to the receiver/dryer inlet pipe (4).
3. Install the receiver/dryer inlet pipe to the receiver/dryer. Secure with the bolt.
4. Connect the pipe fitting at the condenser outlet.
5. Evacuate and recharge the air conditioning (A/C) system. Refer to Refrigerant Recovery and Recharging .
6. Operate the A/C system and inspect for refrigerant leaks. Refer to Leak Testing .