For 1990-2009 cars

## Tail Lamp Replacement 2 Door

### Removal Procedure

1. Remove the 2 screws which secure the tail lamp (5).
2. Pull the tail lamp (5) upward and rearward in order to remove the lamp from the body.
3. Remove the bulb sockets from the tail lamp (5).
4. Remove the tail lamp (5) from the vehicle.

### Installation Procedure

1. Install the bulb sockets to the tail lamp (5).
2. Install the tail lamp (5) to the body. Secure the lamp with the 2 screws.

## Tail Lamp Replacement 4 Door

### Removal Procedure

1. Open the rear-compartment lid.
2. Reposition the rear compartment side trim in order to access the nut that retains the tail lamp.
3. Remove the nut which secures the tail lamp (1).
4. Remove the 2 screws which secure the tail lamp (1).
5. Remove the tail lamp (1) from the body in order to attain access to the bulb sockets.
6. Remove the bulb sockets from the tail lamp (1).
7. Remove the tail lamp (1) from the vehicle.

### Installation Procedure

1. Install the bulb sockets to the tail lamp (1).
2. Install the tail lamp (1) to the body. Secure the lamp with the 2 screws and with the nut.
3. Position the rear compartment side trim back to the original position.
4. Close the rear-compartment lid.