For 1990-2009 cars

1. Loosen the clutch pedal stop lock nut (5)
2. Turn the clutch pedal stop bolt (1) clockwise in order to lower the clutch pedal height.

Adjustment
Clutch pedal height stays within 8 mm (0.3 in) of the brake pedal height.

3. Turn the clutch pedal stop bolt (1) counterclockwise in order to raise lower the clutch pedal height.

Adjustment
Clutch pedal height stays within 8 mm (0.3 in) of the brake pedal height.

4. Tighten the clutch pedal stop lock nut (5).