For 1990-2009 cars

## Transmission Mount Replacement Left

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the following components from the vehicle:

• | The 5 left splash shield retainer clips

• | Remove the left splash shield.

3. Support the transaxle with a suitable hydraulic jack.
4. Remove the two retaining nuts (2) from the left transaxle mount.
5. Remove the through bolt (1) from the left transaxle mount (4).
6. Lower the transaxle slightly until the left transaxle bracket (6) is clear of the left transaxle mounting studs.
7. Remove the left transaxle mount from the vehicle.

### Installation Procedure

1. Install the left transaxle mount into the vehicle.
2. Use a suitable hydraulic jack in order to raise the transaxle into position.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the left transaxle through bolt (1) into the left transaxle mount (4).

Tighten
Tighten the left transaxle through-bolt to 60 N·m (44 lb ft).

4. Install the 2 transaxle mount retaining nuts (2).

Tighten
Tighten the retaining nuts to 60 N·m (44 lb ft).

5. Remove the hydraulic jack.
6. Install the left splash shield onto the vehicle.
7. Use the 5 retainer clips in order to secure the splash shield.
8. Lower the vehicle.

## Transmission Mount Replacement Rear

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Support the transaxle with a suitable hydraulic jack.
3. Remove the rear transaxle mount through bolt (6) and the nut (5).
4. Remove the 2 rear transaxle mount bolts (1).
5. Remove the rear transaxle mount (2).

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the rear transaxle mount (2) into the vehicle.

Use two rear transaxle mount retaining bolts (1) in order to secure the rear transaxle mount (2).

Tighten
Tighten the transaxle retaining bolts to 60 N·m (44 lb ft).

2. Install the rear transaxle mount through bolt (6) and the nut (5).

Tighten
Tighten the rear transaxle mount through bolt and nut to 60 N·m (44 lb ft).

3. Remove the hydraulic jack from under the transaxle.
4. Lower the vehicle.