For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the following components from the front bumper fascia:

• | The five screws (2) which secure the front bumper impact bar

• | The front bumper impact bar (1)

### Installation Procedure

1. Install the front bumper impact bar (1) to the front bumper fascia. Secure the impact bar with the five screws (2).
2. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .