For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Turn the light switch to the PARK position. | The following lamps are on:

• | All the parking lamps

• | The rear side marker lamps

• | The tail lamps

• | The license plate lamps

• | License and Tail Lamps Inoperative

• | Park, Tail and Side Marker Lamps Inoperative

2 |

1. Turn the light switch to the OFF position.
2. Press the hazard switch to the ON position.

The following components flash approximately 80-90 times per minute:

• | The front turn lamps

• | The rear turn lamps

• | The left turn indicators

• | The right turn indicators

• | Tail, Marker, and License Lamps Always On

• | Park, Tail and Side Marker Lamps Inoperative

• | Turn Signal and Hazard Lamps Inoperative

3 |

1. Press the hazard switch to the OFF position.
2. Depress the brake pedal.

The stop lamps illuminate.

Stop Lamps Inoperative

4 | Release the brake pedal. | The stop lamps go out. | Stop Lamps Always On
5 |

1. Turn the ignition switch to the ON position.
2. Press the turn signal switch to the left turn position.

The following components flash approximately 80-90 times per minute:

• | The left front turn lamps

• | The left rear turn lamps

• | The left turn indicator

• | Turn Signal Lamps Inoperative - Left or Right Side

• | Turn Signal Indicators Inoperative - Left Side

6 | Press the turn signal switch to the right turn position. | The following components flash approximately 80-90 times per minute:

• | The right front turn lamps

• | The right rear turn lamps

• | The right turn indicator

• | Turn Signal Lamp Inoperative - Left Side Front or Turn Signal Lamp Inoperative - Right Side Front

• | Turn Signal Indicators Inoperative - Right Side

7 | Press the turn signal switch to the OFF position. | The turn signal lamps stop flashing. |

• | Turn Signal Lamps Always On - One Side

• | Turn Signal Lamps Always On - One Side

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.