For 1990-2009 cars

### Removal Procedure

1. Fold back the carpet and spare tire cover in order to gain access to the rear end interior trim panel plastic retaining clips.
2. Remove the following components from the vehicle:

• | 9 plastic retaining clips

• | The rear end interior trim panel (5)

### Installation Procedure

1. Install the rear end interior trim (5) to the vehicle. Secure the trim with 9 plastic retaining clips.
2. Reposition the rear compartment carpet back to it's original position.