For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the following components from the rear bumper:

2.1. | The 2 screws

2.2. | The license plate lamp assembly (3)

3. Remove the license plate lamp bulb socket (1) from the lamp assembly (3).
4. Remove the license plate lamp bulb (2) from the socket (1).

### Installation Procedure

1. Install the license plate lamp bulb (2) to the socket (1).
2. Install the license plate lamp bulb socket (1) to the lamp assembly (3).
3. Install the license plate lamp assembly (3) to the rear bumper. Secure the lamp assembly with the 2 screws.
4. Connect the negative battery cable.