For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Power Door Locks System Check performed? | -- | Go to Step 2 | Go to Power Door Locks System Check
2 | Test for an open in the BLU/RED wire between the actuator terminal 2 and S308. Was an open found? | -- | Go to Step 4 | Go to Step 3
3 | Test for an open in the BLU wire between the actuator terminal 1 and S307. Was an open found? | -- | Go to Step 4 | Go to Step 5
4 | Repair the open in the wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Door Locks System Check | --
5 | Replace the door lock actuator. Refer to Front Side Door Lock Replacement or to Rear Door Lock Replacement . Is the repair complete? | -- | Go to Power Door Locks System Check | --