For 1990-2009 cars

## Windshield Pillar Garnish Molding Replacement 2 Door

### Removal Procedure

1. Loosen the door opening lace along the windshield side garnish molding (12).
2. Unsnap and remove the windshield side garnish molding (12) from the vehicle.

### Installation Procedure

1. Install the windshield side garnish molding (12) to the vehicle.
2. Press the door opening lace into place along the windshield side garnish molding (12).

## Windshield Pillar Garnish Molding Replacement 4 Door

### Removal Procedure

1. Loosen the door opening lace along the windshield side garnish molding (11).
2. Unsnap and remove the windshield side garnish molding (11) from the vehicle.

### Installation Procedure

1. Install the windshield side garnish molding (11) to the vehicle.
2. Press the door opening lace into place along the windshield side garnish molding (11).