For 1990-2009 cars

### Removal Procedure

1. Remove the screw and the 3 plastic retainers (5) that retain the front wheelhouse panel (2) to the front bumper fascia.
2. Remove the 5 screws (4, 6) that retain the front wheelhouse panel (2) to the front fender (1).
3. Remove the front wheelhouse panel from the vehicle.

### Installation Procedure

1. Install the front wheelhouse panel (2) to the front fender (1). Secure the panel with 5 screws (4, 6).
2. Secure the front wheelhouse panel (2) to the front bumper fascia with the following components:

• | The screw

• | the 3 plastic retainers (5)