For 1990-2009 cars

1. Remove the parking lock pawl shaft (7081) and the spring.
2. Remove the parking lock pawl (7079).
3. Remove the parking lock pawl sleeve (7082) from the transaxle case (7085).
4. Remove the restrictor pin (7084) and the snap ring (7083) from the parking lock pawl sleeve (7082).
5. Remove the nut lock washers (7094,7096).

Remove the manual detent spring assembly (7092).

6. Remove the manual shift shaft (7086).
7. Remove the manual lever locknuts (7091).

Remove the manual shift lever (7090).