For 1990-2009 cars

### Removal Procedure

1. Loosen the 2 clamps on the two EVAP canister surge tank vacuum hoses.
2. Disconnect the 2 vacuum hoses from the EVAP canister surge tank.
3. Remove the 2 screws from the EVAP canister surge tank bracket.
4. Remove the EVAP canister surge tank.

### Installation Procedure

1. Install the EVAP canister surge tank to the bracket on the intake manifold.
2. Secure the EVAP canister surge tank with the 2 screws.
3. Connect the two vacuum hoses to the EVAP canister surge tank.
4. Secure the 2 vacuum hoses with the 2 clamps.