For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Audible Warnings System Check? | -- | Go to Step 2 | Go to Audible Warnings System Check
2 |

1. Disconnect the audio alarm module connector.
2. Turn the light switch to the PARK position or the HEAD position.
3. Use a J 35616-200 in order to probe the audio alarm module connector from cavity 2 to ground.

Does the test lamp light?

--

Go to Step 4

Go to Step 3

3 | Repair the open in the RED/YEL wire between cavity 2 of the audio alarm module and S219. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Audible Warnings System Check | --
4 |

1. Inspect for a poor connection at the audio alarm module.
2. If the connection is OK, replace the audio alarm module. Refer to Audio Alarm Module Replacement .

Is the repair complete?

--

Go to Audible Warnings System Check

--