For 1990-2009 cars

## Body Rear End Adjustment Specifications 2 Door

The following specifications are to be used to ensure the proper clearances and flushness of the rear end body components after body repair procedures are complete.

#### Sheet Metal Tolerances--2-Door Model

Location | Clearance Gap | Flushness
--- | --- | ---
Front door to Quarter Panel (3) | 5.0 mm (0.20 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
Liftgate Door to Quarter Window (2) | 6.3 mm (0.25 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
Liftgate Door to Roof (1) | 8.6 mm (0.34 in) | 0.0 to -1.0 mm (0.00 to -0.04 in)
Liftgate Door to Roof (4) | 5.6 mm (0.22 in) | 0.0 to -1.0 mm (0.00 to -0.04 in)
Liftgate Door to Extension Back Panel (5) | 3.8-5.8 mm (0.15-0.23 in) See Note | --
Liftgate Door to Rear Combination Lamp (6) | 5.2 mm (0.205 in) | 2.5 mm (0.098 in)
Note: Difference of the left and the right side: 1.0 mm (0.04 in) maximum

## Body Rear End Adjustment Specifications 4 Door

The following specifications are to be used to ensure the proper clearances and flushness of the rear end body components after body repair procedures are complete.

#### Sheet Metal Tolerances--4-Door Model

Location | Clearance Gap | Flushness
--- | --- | ---
Rear Door to Quarter Panel (1) | 5.1 mm (0.20 in) | 0.0-1.0 mm (0.00-0.04 in)
Trunk Lid to Quarter Panel (2) | 3.6 mm (0.14 in) | -1.8 to 0.0 mm (-0.07 to 0.00 in)
Trunk Lid to Rear Window (5) | 5.0 mm (0.20 in) | -2.6 mm (-0.102 in)
Trunk Lid to Rear Combination Lamp (4) | 0.3 mm (0.012 in) | --
Trunk Lid to Extension Back Panel (3) | 4.2 mm (0.17 in) See Note | -1.0 to 0.0 mm (-0.4 to 0.00 in)
Note: Difference of the left and the right side: 1.0 mm (0.04 in) maximum