For 1990-2009 cars

# 1990 FRENCH LABEL INSTALLATION INSTRUCTIONS

I. Passenger Cars - Page 1

II. Light Duty Trucks (Diesel Only) - Page 12

III. C/K, P, ST Truck and G and M Vans, Pickup, Trooper - Page 14

IV. Medium Duty Truck (Except "530") Page 21

V. Medium Duty Truck (Topkick "530") Page 24

I. VEHICLES AFFECTED: All 1990 Passenger Cars

Labels are pressure sensitive, therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over their entire surface.

Locate labels next to corresponding English labels, unless otherwise noted. Both labels must be readable.

Engine

1) Fan Caution Label

- If vehicle is equipped with an English label, place label 52350076 over it. Otherwise, place label 52350076 adjacent to the English embossed message on fan shroud. For "R" car use label 52354789, for A, J, F, N or Y car use 52355271 adjacent to English label.

2) Auxiliary Fan Caution Labels.

- If "J or N" car, place label 744759 over English label on fan shroud.

- If "Y" car use 52355272 over English label.

3) Battery Labels

- Place label 52362567 on Sprint (M-Car).

- Place label 52356159 over original label on: A,B,C,H,V,K,E,Y,F,J,N,L.

4) Battery Charge Indicator Label

- Place 52354793-94-95 over the English label (M-R Car) on: R-car.

5) Air Conditioner Compressor/Evaporator Labels

- Place 744775 on: A,B,C,H,V,K,E,Y,J,N,R.

- Place Label 744775 over the words "Refrigerant Oil, Model No.", such that LH edge of overlay is even with LH edge of silver portion of compressor label.

- Place label 52360150 on: Optima T-225 adjacent to English. label.

6) Hood Prop Rod Label

- Place label 52354520 over English label on: L.

7) Engine Oil Fill Cap Label

- Place labels 52355864 or 52355865 (depending on which oil is used, sw or low) over English label on: A,B,C,H,V,K,E,H,F,J,N,L,R.

8) Turbo Engine Oil Recommendations Label

- Place 52362528 on: J,N adjacent to English label.

9) Ignition Switch Notice Label (Cadillac Only)

- Place label 52352902 over English label which is located on top of the battery on: C,H,V,K,E,Y.

10) Vehicle Fluids Identification Label (Cadillac "C" Only)

- Place label 52353411 beside the English label on top of the air cleaner

11) A/C Refrigerant Charging Procedure Label

- Place label 52353413 over the original English label on top of the radiator support on: C,H.

- Place label 52355251 adjacent to English label on: V,K,E,Y.

- Place label 52356186 adjacent to English label on: J,N,L.

12) Notice Electrical System Ignition "Off" warning.

- Place label 52356803 over existing English label on: B,C,H,V,K,E,Y.

13) Radiator Caution Label

- Place label 52354790 adjacent to English label on: R (I-Mark).

14) Composite Headlamp Label

- Place label 52355512 adjacent to English label on: A,C,H,V,K,E,Y,F,J,N,Optima T-225.

15) Fuse Block Identification Label

- Place label 52355488 over the existing English label on: V,K,E,Y.

16) Relay Centre Label

- Place labels 52355500, or 52355504 over existing English labels on: V,K,E,Y.

17) Inflatable Restraint System

- Place label 52360625 adjacent to English label. Place the Blue/White, French Supplemental Inflatable Restraint (S.I.R.) Notice label adjacent to the English label on the fan shroud.

18) Refrigerant Caution Label

- Place 52361685 on: L - adjacent to English label - Place 52360351 on: W - adjacent to English label

19) Caution Wiper, on: U

- Place 52362755 adjacent to existing English label.

20) Accessory Belt Routing Labels

- The Bilingual Label should go directly over top of the English label so that the Bilingual Only shows.

For U.S. No. 10042993 place 52356183 on: A For U.S. No. 22518472 place 52352960 on: A,C,H,J,N For U.S. No. 10044858 place 52356837 on: A,J,N,L,W For U.S. No. 10045371 place 52356812 on: C,H,V,K,E,Y For U.S. No. 10045372 place 52356813 on: C,H,V,K,E,Y For U.S. No. 10045326 place 52356814 on: C,H,V,K,E,Y For U.S. No. 10045365 place 52356815 on: C,H,V,K,E,Y For U.S. No. 25523397 place 52354640 on: J,N For U.S. No. 14076368 place 52356802 on: J,N,L For U.S. No. 10105211 place 52361696 on: V,K,E,Y For U.S. No. 10055889 place 52360073 on: F For U.S. No. 10100036 place 52361585 on: F

21) Battery Catalogue

- Place 52356160 on: A,B,C,H,V,K,E,Y,F,J,N,L over existing label on battery.

22) Special Coolant Fill Label

- Place 52360259 on: W adjacent to English label.

23) HDLP Bulb Replacement Inst.

- Place 52356207 on: J,N adjacent to English label.

24) Brake Fluid Pressure Caution (ABS)

- Place 52361684 on: A,C,H,V,K,E,Y adjacent to English label.

25) Notice Dextron II Only

- Place 52362564 on: M (Sprint) adjacent to English label.

26) Caution Active Ride Suspension

- Place 52362571 on: V,K,E,Y adjacent to English label 10140793.

27) Caution Frt. Susp. Gas Under Pressure

- Place 52362570 on: V,K,E,Y adjacent to English label 10140794.

28) Caution Fuel Flammable

- Place 52362963 on all vehicles - Label to be wrapped around fuel line adjacent to English label. If no English labels present, there is no need to use the French. (4 per unit)

Passenger Compartment

1) Owner's Manual Reference Label (All Vehicles)

- On: A,B,C,H,V,K,E,Y,F,J,N,M,Optima,W,R place label 745764 on trailing edge of door adjacent to Tire and Certification Labels.

2) Manual Transmission Shift Indicator Light Label

- Place label 52353708 adjacent to English label on LH Sunvisor on: A,F,J,N.

3) Twilight Sentinel Label and Tag (If Vehicle So Equipped)

- Place label 744673 on Amp Unit (under Dash, Driver's Side) over existing label, such that Model No. shows on: A,B,C,K,E,Y.

- Place tag 744645 or 52354600 on shaft of light switch adjacent to English tag. 744645 on: A,B,V,K,E,Y 52354600 on: C,H

4) Fuse Block Identification Labels ("C" Cars Only)

- Remove the fuse block cover and install label 52353407 (Olds), 52353408 (Buick), or 52353409 (Cadillac), over the fuse identification chart on the inside surface of the fuse block cover (C-H Cars).

- Place labels 52355486 (Cadillac) and 52355487 (Olds) over existing English label on: V,K,E,Y.

- Place label 52354798 over existing English label (R Car)

- Place label 52360260 over existing English label (L-Car)

- Place label 52354729 over existing English label (J-N Car)

5) Headlight Flash to Pass Signal Switch Tag (Pontiac "A" with Y88 Package Only)

- Place tag 52352651 on shaft of signal switch adjacent to English tag

6) Roof Panel Notice Label (Corvette Only)

- Place label 52350964 on left and right side roof panels over English labels.

7) Anti-theft (used on Window, comes in Glove Box)

- Place 52360255 in glove box of vehicle.

8) Start Procedure Labels

Place Label 52355180 adjacent to 14086559 on: B,J,N Place Label 52355181 adjacent to 14086560 on: A,F,J,N Place Label 52356246 adjacent to 10045066 on: J,N Place Label 52356247 adjacent to 14076411 on: J,N Place Label 52355183 adjacent to 14086562 on: F Place Label 52354635 adjacent to 25523211 on: A,C,H,J,N Place Label 52354732 adjacent to 25523894 on: A,C,H,V,K,E,Y Place Label 52354569 adjacent to 14086559 on: F 52360219: J,N 52362589: Optima

9) All Wheel Drive Instruction on: A,W

- Place label 52361596 adjustment to existing English label

10) Instruction Sheet Sunroof Crank Label On: B

- Place instruction sheet 52354062 in glove box

11) Dual Mode Retractor Child Restraint Seat Belt Label on: C,H (2 per job)

- Wrap label 20584675 around D-ring side of belt directly around stitched area.

12) Childproof Lock Label

- Place label 52354792 directly over English label on: Passport Isuzu 760JRT Impulse or Stylus, R.

13) Extension Spa Whl Stowage Label (J-N Car) (In Glove Box)

- Place label 52355166 on Extension adjacent to English label.

14) Ash Tray Retainer Label

- Place label 52355313 adjacent to English label on: R.

15) Relay Centre Label (In console)

- Place label 52355503 over English label 25522931 on: V,K,E,Y

- Place label 52355501 over English label 25522933

16) Anti Lock Brake Label

- Place card 52355499 under straps on RH S/Shade for Pontiac STE on: A

17) Tire Sensor Label

- Place 52356861 adjacent to 14102346 on: Y (Quantity 4).

18) INST Sheet Hub-Cap Installation

- Place sheet 52360389 in glove box on: C,H.

19) Anti-Theft Locking System

- Place label 52360256 adjacent to existing English label on: L,W

20) Radio Theft Deterent

- Place 52356797 on: A - adjacent to English label if English label is used. Otherwise, put in glove box.

21) Caution Seat Code A,B,C.

- Place 52352748, 49, 50 on: U Car - adjacent to English label

22) Scotchguard

- Place 52362770 on: A,B,V,K,E,Y,F,U,J,N,M,L,W - Put on windows of cars with cloth interiors (adjacent to English label)

23) Roof Lift Off Windows Storage Instructions (T-Roof)

- Place 52362754 on: F (Qty - 2) adjacent to English label

24) Jack Location Label - Place 52362768 on: Y - adjacent to English label

25) Shock Absorber Caution Label (4 per vehicle)

- Place 52353504 on: V,K,E,Y adjacent to English label

26) Automatic Headlamp Dimmer Sensor

- Place 744683 on: V,K,E,Y

27) Place the French Supplemental Inflatable Restraint System Sunshade Warning label adjacent to the English verson.

28) Place the three yellow, French Supplemental Inflatable Restraint System Caution labels in the following locations:

1) on the fan shroud adjacent the Blue/White French S.I.R. Notice label,

2) under the neck of the steering column,

3) on the front passenger door pillar.

Trunk

1) Jack Instruction Labels

- Place adjacent to English labels

- Place 52350162 on: B wagons

- Place 52350163 on: B sedans

- Place 52362765 on: Y Place 52362766 Place 52362767 on: Y & ZR1 wheel stowage

- Place 746164 Place 52355478 on: E Place 52355479 Place 52355480

- Place 52350162 on: V Place 52360057

- Place 52362586 on: F Place 52361463 on: F - Stowage GTA

- Place 52362534 on: V

- Place 52355477 on: J,N

- Place 52362563 on: M - Place 52362569 on: Stowage

Place 52362530, 52362531 on: Passport Isuzu 760 JRT Impulse or Stylus

If "A" Station Wagon, remove the RH quarter panel trim cover and place label 52361461 beside the English label.

If "R" car, place label 52354796 adjacent to English label.

If "L", place label 52361510 adjacent to English label.

If "C-H", place label adjacent to English label, 52361491 (CAD) 52361492 (Buick-Olds-Pont)

If "W" Car, place 52362320 adjacent to English label

Daewoo-T place 52360094 adjacent to English label.

2) Jack Assembly Labels

- If side mounted jack, place appropriate label 746123, 52354515, 52354509, 52351308, 52353402, 52353404 on side opposite to corresponding English label.

- For " R " car, place 52354797 over English label, and 52354791 adjacent to English label.

- If bumper jack, place label 746124 over English label on jack base.

- For Daewoo-T place 52360095 adjacent to English label

- For "W" car place 52362137 adjacent to English label Jack Assembly Caution Label (SUP)

- Place 52356209 on: F-car on Jack

- Place 52362566 on: M-car on Jack

3) Wire Wheel Cover Lock Removal Label (If vehicle so equipped)

- Place label 746197 or 52353419 adjacent to English label on trunk lid.

- Place 746197 on: A,B,C,K,E,Y

- Place 52353419 on: A,C,H,W

- 52361679 for W car only

4) Roof Panel Stowage Instruction Label ('F' Car only)

- Place label 52354086 adjacent to English label on the roof panel stowage bag.

5) Space Saver Spare Tire ("F" Car only)

- Remove tire and inflation canister.

- Place label 52350966 on rim next to original label.

- Place label 746415 over original label on canister so that information shows through the 3 windows. To do this, line up top of label with top of original label and right hand side of label flush with original label.

6) Jack Locater Labels

- Place 52361462 over existing English label on: W Car

- Place 52362568 on: M Car.

7) Inflation Canister Label

- Place 746415 on: F Car.

8) Electric Lock Fuel Cap Label (If vehicle so equipped)

- Place label 52352880 on fuel cap opposite to English label on: B,C,H,V,E,K,Y

9) Fuel Filler Door Manual Release Label

- Place label 52353416 or 52355250 beside the English label on the inner surface of the rear trunk lid flange on: C,H,V,K,E,Y.

10) Tailgate Transfer Decal ("A" Station Wagons only)

- Place decal 52353624 below the English decal which is located just above the tailgate door lock (Note: French decal should be positioned below the lock cylinder).

11) Remote Locking Fuel Door Label

- Place label 52351460 on bumper filler panel adjacent to English label on: C,H,V,K,E,Y.

12) Full Size Flat Aluminum Wheel Stowage (A Car)

- Place label 52354613 adjacent to English label.

13) Jack Instruction Location Label

- Place label 52353417 on compartment lid adjacent to English label on: C,H.

14) Centre Hub Cap Removal Instruction

- Place label 52354730 adjacent to English label on: J,N.

15) Trailer Towing Notice Label

- Place label 52355167 adjacent to English label on: V,K,E,Y.

16) Station Wagon Third Seat Release

- Place 744742 on: B car adjacent to English label.

17) Cargo Cover Label

- Place 744774 on: A car adjacent to English label

18) Spare Caution Label (Compact and Regular)

- Place 52353513 on: A,B,C,H,V,K,E,F,J,N,L,W

- Place 52362143 on: A

- Place 52353291 on: Y

All adjacent to English label

19) Jack Pad Filler Location

- Place 52360931 on: W car adjacent to English label

20) Remove and discard all extraneous Enqlish advertising. Labels which are released late will be added to this attachment when the installation instructions are reissued.

II. VEHICLES AFFECTED: 1990 Light Duty Trucks (Diesel only)

General Information

Labels are pressure sensitive; therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over the entire surface.

Locate labels next to English labels, unless otherwise noted. Both labels should be readable.

Engine Compartment

1) Dual Battery Labels (Lt. Duty Truck Only)

- Follow same instructions for extra battery (diesel engine) as for single battery (gasoline engine) as outlined in the general instructions in the Product Service Bulletin.

2) Oil Filler Cap Label

Place label 52355864, 52355865 over one of the original labels on the oil filler cap. (Key on Oil required) on: Diesel (LD Truck), RVP Truck, G-Van, M-Van, S/T Truck, CK Truck.

3) Diesel Fuel Filter Labels

- Place label 74944A over English label on the secondary fuel filter.

- Place label 745944B over English label on the primary fuel oil filter.

4) Maximum Voltage Caution

- Place label 52354639 adjacent to English label on: Diesel (LD Truck).

5) Battery Caution Label

- Place 52356159 on: Diesel (LD Truck)

6) Diesel Engine Label Sheet

- Place 744667 on: Diesel (LD Truck)

7) Battery Catalogue Number

- Place 52356160 on: Diesel (LD Truck)

III. VEHICLES AFFECTED: 1990 C/K, P, S/T Truck and G and M Vans, Pickup, Trooper

Labels are pressure sensitive; therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over the entire surface.

Locate labels next to English labels, unless otherwise noted. Both labels should be readable.

Engine

1) Fan Caution Label

- Place 52362522 and 52362525 on: Tracker adjacent to English label.

- If Vehicle is equipped with an English label, place label 52350076 over it on: RVP Truck, G-Van, M-Van, S/T Truck.

- Place label 52355271 adjacent to English label on: RVP Truck.

- Place 52356159 on: Diesel (LD Truck), M-Van, S/T Truck, CK Truck and two on: RVP Truck, G-Van.

- Place label 52355271 adjacent to English label on: RVP Truck.

2) Battery Caution Labels

- Place 52356338 over English Label (Pickup and Trooper Trucks).

- Place 52356159 on: Diesel (LD Truck), M-Van, S/T Truck, CK Truck and two on: RVP Truck, G-Van.

- If vehicle is equipped with auxiliary batteries (LH front corner of CK Truck, under driver seat on G-Van), locate additional labels as per above instructions.

3) - Battery Charge Indicator Label

- Place 52362523 on: Tracker

4) Battery Catalogue Number

- Place 52356160 on: RV, P, G-Van, M-Van, ST, CK, Trucks adjacent to English Labels.

5) Battery and Cable Installation

- Place 52362147 on: ST Truck adjacent to English Labels.

6) Caution Fuel Flammable

- Place four 52362963 on every vehicle. Use labels (4) adjacent to English labels. If no labels present (metal fuel lines) do not use labels. - Label should be wrapped around fuel line.

7) Air Conditioner Compressor/Evaporator Labels

- Place label 744775 over the words "Refrigerant Oil, Model No.", such that LH edge of overlay is even with LH edge of silver portion of compressor label.

- Place label 744775 adjacent to corresponding English label on compressor.

- Place label 744775 adjacent to corresponding English label on evaporator.

8) Air Cleaner Labels

- Place 52356340 over existing English label (Pickup and Trooper Trucks).

9) Oil Filter Label

- Place label 744750 or 746827 (whichever is appropriate) on oil filter canister adjacent to original label.

10) Hood Prop Rod Label (S-T Truck, M-Van)

- Place label 52354520 over original English label.

11) Engine Oil fill Cap Label

- Place label 52355864, 52355865 over original English label on the oil fill cap (key on type of oil required) on: Diesel (LD Truck), RVP Truck, G-Van, M-Van, ST Truck, CK Truck.

12) Jack Instruction Labels (CK Truck)

- Place label 52362825 on RH wheelwell in engine compartment on flat visible location adjacent to corresponding English label.

13) Jack Assembly Label (CK Truck)

- Place label 746125 over English label on jack assembly.

14) A/C Refrigerant Charging Procedure Label

- Place 52356198 on: RV, P Trucks adjacent to English label.

15) Caution Hot Surface - Place directly on top of existing English Label

- Place 52361669 on: S/T Truck

16) Coolant Service Notice Label

- Place 52356343 adjacent to English Language Label on: Passport Pickup and Trooper Truck.

17) Refrigerant Caution Label

- Place 52356341 adjacent to existing English Label. (Pickup & Trooper Trucks).

- Place 52362521 and 52362524 on: Tracker.

18) Rad Caution Label

- Place 52356339 over existing English Label (Pickup & Trooper Trucks)

19) Accessory Belt Routing Label

Use 52362145 in place of on: M-Van Use 52362146 in place of on: M-Van Use 52356812 in place of 10045371 on: RV, P, CK, G-Van Use 52356813 in place of 10045372 on: RV, P, CK, G-Van Use 52360932 in place of 10085701 on: RV, P, ST Use 52361584 in place of 10085749 on: RV, P, M-Van, ST, CK Use 52356814 in place of 10045326 on: G-Van, M-Van, CK Use 52356242 in place of 10048664 on: ST Use 52360631 in place of 10100080 on: ST Use 52356314 in place of 15547741 on: CK Use 52356315 in place of 15547740 on: CK Use 52362321 in place of on: G-Van, M-Van, CK

- Place bilingual label over existing English label. (If label is French language only, place adjacent to Engish label).

Passenger Compartment

1) Transfer Case Shift Label

- With LH sunvisor in down position, remove the English transfer case shift label.

- If "RV, P" Truck, place label 52350175 on LH sunvisor in down position, and locate label in centre of sunvisor.

- If "ST" Truck, place label 52352672 on LH sunvisor in down position, and locate label in centre of sunvisor.

2) Owner's Manual Reference Label

- Place label 745765A on trailing edge of driver's door in proximity to the certification label.

- If "C,K,M,P,S,T" Truck, and equipped with camper option, place label 745765B on glove box door near the camper loading label 338601 also on: RV.

3) New Engine Origin Label

- Place label 746246 adjacent to corresponding English label for L25 engine on LH side door.

- Place label 52351461 adjacent to corresponding English label for LRI engine on LH side door.

4) Roof Rear Bolt Removal Label (CK Truck)

- If Jimmy/Blazer with hardtop cap, place label 746000 over corresponding English label at rear RH corner.

5) Jack Instruction Label (G Van)

- Place on opposite side to English.

- With option AQ4, place label 52354518 over bottom section of label 52354519.

6) Jack Assembly Label (S-T Truck)

- Place label 52351773 on side opposite to English label on jack asm.

7) Shock Absorber Caution Label ("T" Truck Only)

- If vehicle is equipped with option Z71, raise vehicle on a hoist and install labels 52353504 adjacent to the original English labels on the shafts of each shock absorber.

8) Engine Cover Removal Label (M-Van)

- Place label 52354517 over existing English label in glove compartment area.

9) Jack Caution Label (M-Van)

- Place 52354513 adjacent to existing English label.

10) Jack Instruction Label (M-Van)

- Install 52360428 similarly to English label and adjacent to it.

11) Jack Instruction Labels (ST Truck)

- Place 52360257 - (03-53) adjacent to English label.

- Place 52360258 - (16) adjacent to English label.

- Place 52362611 - (06) adjacent to English label.

12) Utility Vehicle Handling (ST Truck - RVP Truck)

- Place label 52354648 adjacent to existing English label.

13) Commercial Trailering Label

- Place label 52355329, 52355330 or 52355331 adjacent to English label with corresponding weight on: RV, P Trucks.

14) Windshield Washer Instruction

- Place 52356344 over existing English Label (Pickup)

- Place 52356598 over existing English label (Trooper).

15) 4 Wheel Drive Instruction

- Place 52356600 adjacent to existing English label.

16) Fldg 2nd St Instruction

- Place 52356601 adjacent to existing English label (DLX Trim)

- Place 52356624 adjacent to existing English label (LS Trim)

17) Jack Instruction Label (Pickup and Trooper)

- Place 52356342 adjacent to existing English label (Pickup)

- Place 52356597 adjacent to existing English label (Trooper)

18) Jack Assembly Caution Label (Label on Jack)

- Place 746125 and 52355476 on: RV, P Truck

- Place 746125 outer English label on jack assembly on: G-Van

- Place 52362138 on: CK Truck

- Place 52362520 on: Tracker

19) Jack Instruction Labels (Adjacent to English Label)

- Place 52362825 on: RV, P Trucks

- Place 52354518 and 52362529 on: G-Van

- Place 52362519 on: Tracker (tag)

20) Tailgate Pull (Trooper Truck)

- Place 52356602 over top of existing English label.

21) Glovebox

- Remove and discard all literature or advertising for which a French equivalent does not exist.

22) Engine and Diesel Engine Start Procedure Label

- Place 52356886 on: CK Truck. Place adjacent to English label.

23) Childproof Lock Label

- Place 52362462 on: Trooper truck adjacent to English label.

24) Dual Mode Retractor Child Restraint Seat Belt Label

- Place 20584675 on: ST Truck (2 per job). Wrap around belt at stitching.

25) 4 x 4 Transfer Case Information Label

- Place 52355163 on: ST Truck adjacent to English label.

26) Unleaded Fuel Dash Label

- Place 52356603 on: Trooper truck on top of existing English label.

27) Label Electrical Ground Strap

- Place 52362148 on: P Truck adjacent to English label.

28) Label - Caution Washer Solvent

- Place 52362589 on: Trooper truck on rear washer container.

29) Light Support Bar Caution Label

- Place 52362144 on: ST Trucks adjacent to English label.

30) Lock Free

- Place 52356788 on: Trooper Truck adjacent to English label

31) Cautioin Fuel Spray Label

- Place 52362319 on: P Truck adjacent to English label.

IV. VEHICLES AFFECTED: 1990 Medium Duty Truck (Except "530")

(1989 Packages should be retained and used for this truck. It will be cancelled by December 1. A new "530" MD Truck will have its own new label package which will be added to this bulletin later).

Labels are pressure sensitive; therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over the entire surface.

Locate labels next to English labels, unless otherwise noted. Both labels should be readable.

Engine Compartment

1) Battery

- Place label 52350963 (long, narrow label) over original such that replacement code (bottom RH corner) is visible.

- Place label 52354601 or 52354602, (whichever is appropriate), over original English charge indicator label.

- If 1110, 1150, 1200 battery, place label 744779 over original, such that test indicator, cat. no., etc., are visible.

2) Air Cleaner

- Place label 744678 over original label so that code in top corner is not covered.

- If equipped with a Donaldson air cleaner, place label 746005 over original such that air cleaner, main element, and safety element numbers, are visible.

- If equipped with a United air cleaner, place label 744675 (dry-MD Truck), or 745998 (oil bath-MD/HD), adjacent to original label. If equipped with dry type on HD Truck, place label 744766 over original such that air cleaner and element part numbers are visible.

- If equipped with a Fram air clearner, place label 745999 over original such that assembly and filter replacement part numbers are visible.

3) Air Conditioning Compressor

- Place small tab section of label 744775 (744775C) over the words "Refrigerant Oil, Model No.", such that LH edge of overlay is even with LH edge of original label.

- If unit has a large square label, place "Attention" portion 744775B beneath the English "Caution" note.

- If unit has long, narrow label, place the "Attention" protion 744775A on a flat visible surface on the compressor.

- If equipped with a sleeper compartment label, place label 746421 over existing label.

4) Oil Filter Label

- If equipped with PF-932 type, place label 744746 on oil filter canister adjacent to original label.

- If equipped with PF-35 type, place label 744750 on oil filter canister adjacent to original label.

- If equipped with PM-13-10 type, place label 746417 over original such that part number and type are visible.

5) Fuel Filter Label

- If equipped with AC T-60, T-58 type filters, use label 746416 and place 746416A over primary original and 746416B over secondary original, such that fuel filter numbers are visible.

- If equipped with GF-62T type, place label 745939 over original such that fuel filter type is visible.

- If equipped with AC T-915, T-916 type filters, use label 745944 and place 745944B over primary original and 745944A over secondary original, such that oil filter and replacement types are visible.

6) Coolant Filter Label

- If equipped with type WF-100, place label 744782 completely over the original.

Cab Compartment

1) Instrument Panel Controls

If equipped with:

a) axle shift switch label, place label 746059 over the original.

b) engine stop light label, place label 744785B over the original.

c) choke control label, place label 744785A over the original

V. VEHICLES AFFECTED: 1990 Medium DutyTruck (Topkick "530")

Labels are pressure sensitive; therefore, surfaces must be clean, dry, warm, and free of contaminants, before labels are affixed. Labels must be pressed firmly over their entire surface.

Cab

1) Shift Instruction Label

Place French label beside existing English label on headliner as follows:

Automatic Trans

Use 52363057 adjacent 2018123 Use 52363053 adjacent 716500

Manual Trans

Use 52363113 adjacent 703198 Use 52363059 adjacent 703199 Use 52363050 adjacent 15504169

If equipped with two speed rear axle

Use 52363054 adjacent 1550440 Use 52363112 adjacent 2011705

2) Diesel Engine Equipped Vehicles:

Diesel engine Starting procedure

Place 52363058 adjacent 15656392 on sunshade

Diesel start fluid warning

Place 52363052 adjacent 22514721 on sunshade

3) Daytime running Lights

Place 52362143 over 15614569 on instrument panel

Engine Compartment

4) Ether Start Notice

Place 52363056 adjacent 15656393 on air cleaner

Chassis

5) Clutch Caution

Place 52363051 on back of tag 690623 on bell housing at transmission

6) Notice Avoid Drilling

Place 52362153 adjacent 15614536 on frame rail

7) Place 52362963 adjacent caution label on fuel line (6 labels)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.