For 1990-2009 cars

### Removal Procedure

1. Remove the IP center trim bezel. Refer to Instrument Panel Center Trim Panel Replacement .
2. Gently lift and pull the ashtray guide (1) from the IP center trim bezel (2).

### Installation Procedure

1. Install the ashtray guide (1) to the IP center trim bezel (2).
2. Install the IP center trim bezel. Refer to Instrument Panel Center Trim Panel Replacement .