For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the system check? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 |

1. Turn the ignition switch to the ON position.
2. Move the front wiper/washer lever to the LO position.
3. Backprobe the front wiper motor connector with a test lamp from cavity 2 to ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in SIR. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
4 | Replace the front wiper motor. Refer to Windshield Wiper Motor Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --