For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the parking brake lever trim bezel. Refer to Instrument Panel, Gages and Console in Body and Accessories.
3. Disconnect the parking brake switch electrical connector.
4. Remove the one screw holding the parking brake switch (2) to the parking brake lever (1) assembly. Remove the parking brake switch (2).

### Installation Procedure

1. Install the parking brake switch (2) to the parking brake lever (1) assembly. Secure the switch with one screw.
2. Connect the parking brake switch electrical connector.
3. Install the parking brake lever trim bezel. Refer to Instrument Panel, Gages and Console in Body and Accessories.
4. Connect the negative battery cable.