For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (IP). Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges, and Console.
2. Remove the following components from the IP:

• | The 3 screws

• | The defroster nozzle (13)

• | The left side demister duct (16)

• | The right side demister ducts (4)

3. Remove the following components from the IP:

• | The 1 screw

• | The left side vent duct (15)

• | The right side vent duct (5)

• | The center vent duct (14)

4. Remove the left (15) and right (5) vent ducts from the center vent duct (14) (if necessary).

### Installation Procedure

1. Install the left and right vent ducts to the center vent duct (if necessary).
2. Install the following components to the IP:

• | The 1 screw

• | The left vent duct (15)

• | The right vent duct (5)

• | The center vent duct (14)

3. Install the following components to the IP:

• | The defroster nozzle (13). Secure the nozzle with the 3 screws.

• | The left demister duct (16)

• | The right demister ducts (4)

4. Install the IP. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges, and Console.