For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Exterior Lights System Check performed? | -- | Go to Step 2 | Go to Exterior Lights System Check
2 | Are the right side turn signal lamps inoperative? | -- | Go to Step 3 | Go to Step 4
3 |

1. Turn the ignition switch to the ON position.
2. Move the turn signal switch to the RIGHT turn position.
3. Backprobe the junction block connector C3 with a test lamp from cavity 1 to ground.

Does the test lamp light?

--

Go to Step 5

Go to Step 6

4 |

1. Turn the ignition switch to the ON position.
2. Move the turn signal switch to the LEFT turn position.
3. Backprobe the junction block connector C3 with a test lamp from cavity 2 to ground .

Does the test lamp light?

--

Go to Step 5

Go to Step 6

5 | Replace the junction block. Is the repair complete? | -- | Go to Exterior Lights System Check | --
6 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in SIR. Is the repair complete? | -- | Go to Exterior Lights System Check | --