For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the rear wiper/washer system check performed? | -- | Go to Step 2 | Go to Wiper/Washer Rear System Check
2 |

1. Disconnect the junction block connector C8.
2. Turn the ignition switch to the ON position.

Does the rear wiper motor operate?

--

Go to Step 3

Go to Step 4

3 |

1. Turn the ignition switch to the LOCK position.
2. Disconnect the rear wiper/washer switch connector.
3. Turn the ignition switch to the ON position.

Does the rear wiper motor operate?

--

Go to Step 6

Go to Step 5

4 | Replace the rear wiper motor. Refer to Rear Window Wiper Motor Replacement . Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
5 | Test for a short to voltage in the BLU/GRN wire between the rear wiper/washer switch and rear wiper motor. Was a short to voltage found? | -- | Go to Step 8 | Go to Step 7
6 | Repair a short to voltage in the ORN wire between the rear wiper/washer switch and the rear wiper motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
7 | Replace the rear wiper/washer switch. Refer to Rear Window Wiper and Washer Switch Replacement . Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
8 | Repair the short. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --