For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 23 N·m | 17 lb ft
Clutch Cable Bracket Bolts | 28 N·m | 21 lb ft
Clutch Release Lever Bolt and Nut | 23 N·m | 17 lb ft
Extension Rod Retaining Nut | 40 N·m | 29 lb ft
Flywheel Cover Bolts | 20 N·m | 15 lb ft
Gearshift Control Lever Guide Plate Bolts | 10 N·m | 89 lb in
Gearshift Control Lever Housing Nuts | 6 N·m | 53 lb in
Gearshift Control Lever Housing-to-Guide Plate Nuts | 40 N·m | 29 lb ft
Gearshift Control Shaft Front Through Bolt and Nut | 20 N·m | 15 lb ft
Gearshift Control Shaft Joint Through Bolt and Nut | 20 N·m | 15 lb ft
Gearshift Control Shaft Rear Through Bolt and Nut | 20 N·m | 15 lb ft
Gearshift Guide Case Bolts | 12 N·m | 106 lb in
Gearshift Interlock Bolt | 28 N·m | 21 lb ft
Gearshift Yoke Bolt | 28 N·m | 21 lb ft
Left Case Cover Bolts | 12 N·m | 106 lb in
Left Transaxle Mount Bracket Bolts | 60 N·m | 44 lb ft
Left Transaxle Mount Retaining Nuts | 60 N·m | 44 lb ft
Left Transaxle Mount Through Bolt | 60 N·m | 44 lb ft
Rear Transaxle Mount Retaining Bolts | 60 N·m | 44 lb ft
Rear Transaxle Mount Through Bolt and Nut | 60 N·m | 44 lb ft
Right Case-to-Engine Block Mounting Bolts | 60 N·m | 44 lb ft
Speedometer Driven Gear Case Retaining Bolt | 7 N·m | 62 lb in
Starter Motor Retaining Bolts | 28 N·m | 21 lb ft
Transaxle Drain Plug | 21 N·m | 15 lb ft
Transaxle Hanger Bolt | 12 N·m | 106 lb in
Transaxle Oil Lever/Filler Plug | 21 N·m | 15 lb ft
Transaxle Side Cover Bolts | 12 N·m | 106 lb in