For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Junction Block | Behind the left side of the IP | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
LH Front Speaker | The left front door behind the door trim panel | Entertainment Component Views | Entertainment Connector End Views
LH Rear Speaker (2-Door) | The left rear quarter trim panel | -- | Entertainment Connector End Views
(4-Door) | The rear-window shelf, on the left side | Entertainment Component Views | Entertainment Connector End Views
Radio | The center of the IP | -- | Entertainment Connector End Views
RH Front Speaker | The right front door, behind the door trim panel | Entertainment Component Views | Entertainment Connector End Views
RH Rear Speaker (2-Door) | The right rear quarter trim panel | -- | Entertainment Connector End Views
(4-Door) | The rear-window shelf, on the right side | Entertainment Component Views | Entertainment Connector End Views
C203 (13 Cavities) | The IP harness to the floor harness, behind the left side of the IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C214 (2 Cavities) | The IP harness to the jumper harness of the left front speaker, behind the left kick panel | Harness Routing Views in Wiring Systems | --
C215 (2 Cavities) | The IP harness to the jumper harness of the right front speaker, behind the right kick panel | Harness Routing Views in Wiring Systems | --
C400 (10 Cavities) (4-Door) | The floor harness to the luggage-compartment harness, on the left front side of the luggage compartment near the left-rear speaker | Harness Routing Views in Wiring Systems | --
G202 | The right side of the center IP behind the radio | Harness Routing Views in Wiring Systems | --
P500 | The left front door | -- | --
P600 | The right front door | -- | --
S222 | The IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC -OBD2) breakout | Harness Routing Views in Wiring Systems | --
S224 | The IP harness, approximately 5 cm (2 in) from the data link connector - (DLC -OBD2) breakout | Harness Routing Views in Wiring Systems | --
S237 | The IP harness, approximately 10 cm (4 in) from the radio-connector breakout | Harness Routing Views in Wiring Systems | --
S238 | The IP harness, approximately 3 cm (1.19 in) from the blower-motor connector breakout | Harness Routing Views in Wiring Systems | --
S243 | The IP harness, approximately 5 cm (2 in) from the cigar-lighter connector breakout | Harness Routing Views in Wiring Systems | --