For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Exterior Lights System Check? | -- | Go to Step 2 | Go to Exterior Lights System Check
2 |

1. Turn the ignition switch to the ON position.
2. Move the turn signal switch to the right turn position.
3. Using J 35616-200 backprobe the junction block connector C3 from cavity 1 to ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Replace the junction block. Is the repair complete? | -- | Go to Exterior Lights System Check | --
4 | Replace the combination switch. Is the repair complete? | -- | Go to Exterior Lights System Check | --