For 1990-2009 cars

Condition | Possible Cause
--- | ---
The vehicle exhibits difficult shifting. |

• | Inspect the transaxle oil level in order to verify sufficient lubricant levels.

• | Inspect the clutch pedal free travel for misadjustment.

• | Inspect the clutch disc for distortion or wear.

• | Inspect the pressure plate for wear or weak return springs.

• | Inspect the synchronizer rings for wear or damage.

• | Inspect the gearshift control shaft bushings for worn or damaged bushings.

• | Inspect the transaxle shift shaft for distortion or bending.

Broken or Damaged Engine and Transmission Mounts