For 1990-2009 cars

### Removal Procedure

1. Remove the rear door window. Refer to Rear Side Door Window Replacement .
2. Remove the 6 mounting screws (1) that retain the regulator.
3. Slide the window regulator through the large opening in the door panel.
4. Inspect the gear and the spring for wear and damage.

### Installation Procedure

1. Apply a multipurpose grease to all lubrication and sliding points on the regulator (1), as indicated by the arrows.
2. Install the window regulator to the door. Secure the regulator with 6 mounting screws (1).
3. Install the rear door window. Refer to Rear Side Door Window Replacement .