For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor Belt Tensioner Lock Nut | 45 N·m | 33 lb ft
A/C Low Side Bracket Bolt | 15 N·m | 11 lb ft
Battery Cable Nut | 15 N·m | 11 lb ft
Camshaft Housing Bolts | 11 N·m | 97 lb in
Camshaft Sensor Housing Bolts | 11 N·m | 97 lb in
Camshaft Timing Sprocket Bolt | 60 N·m | 43 lb ft
Connecting Rod Bearing Cap Nuts | 35 N·m | 26 lb ft
Coolant Pump Mounting Nuts and Bolts | 13 N·m | 115 lb in
Coolant Pump Pulley Bolts | 11 N·m | 97 lb in
Coolant Return Pipe Bolts | 20 N·m | 15 lb ft
Crankshaft Pulley Bolts | 16 N·m | 12 lb ft
Crankshaft Timing Sprocket Bolt | 130 N·m | 94 lb ft
Cylinder Head Bolts | 68 N·m | 49 lb ft
Valve Rocker Arm Cover Bolts | 11 N·m | 97 lb in
Engine Oil Drain Plug | 35 N·m | 26 lb ft
Engine Oil Pan Bolts and Nuts | 11 N·m | 97 lb in
Exhaust Manifold With PUP | 32 N·m | 24 lb ft
Exhaust Manifold Without PUP | 23 N·m | 17 lb ft
Exhaust Manifold Stiffener Bracket Bolts | 50 N·m | 37 lb ft
Flywheel Retaining Bolts: Automatic Transaxle Equipped Vehicles | 95 N·m | 69 lb ft
Flywheel Retaining Bolts: Manual Transaxle Equipped Vehicles | 78 N·m | 57 lb ft
Front Pipe/Catalytic Converter Assembly-to-Exhaust Manifold Bolts | 50 N·m | 37 lb ft
Front Pipe/Catalytic Converter Assembly-to-Resonator/Center Pipe Nuts | 35 N·m | 26 lb ft
Generator Cover Plate Bolts | 10 N·m | 89 lb in
Generator Mounting Bolts and Nuts | 23 N·m | 17 lb ft
Guide Tube Bolts | 11 N·m | 97 lb in
Heat Shield Bolts | 15 N·m | 11 lb ft
Intake Manifold Mounting Bolts and Nuts | 23 N·m | 17 lb ft
Main Bearing Cap Bolts | 54 N·m | 40 lb ft
Oil Pressure Switch | 14 N·m | 10 lb ft
Oil Pump Mounting Bolts | 11 N·m | 97 lb in
Oil Pump Strainer Bolt | 11 N·m | 97 lb in
Oil Pump Strainer Bracket Bolt | 11 N·m | 97 lb in
Rear Engine Mount Frame Bracket-to-Frame Bolts | 55 N·m | 41 lb ft
Rear Engine Mount Connecting Bracket-to-Rear engine Mount Frame Bracket Nuts | 55 N·m | 41 lb ft
Rear Engine Mount-to-Engine Bracket Nut | 55 N·m | 41 lb ft
Rear Engine Mount-to-Bulkhead Bolts | 55 N·m | 41 lb ft
Rear Engine Mount-to-Engine Bracket-to-Engine Bolts and Nut | 55 N·m | 41 lb ft
Rear Engine Mount Through Bolts and Nut | 55 N·m | 41 lb ft
Rear Main Seal Housing Bolts | 11 N·m | 97 lb in
Resonator/Center Pipe-to-Front Pipe/Catalytic Converter Assembly Nuts | 35 N·m | 26 lb ft
Right Engine Mount Through Bolt | 55 N·m | 41 lb ft
Right Engine Mount-to-Mounting Bracket Bolts | 55 N·m | 41 lb ft
Rocker Arm Shaft Bolts | 11 N·m | 97 lb in
Timing Belt Cover Nut and Bolts | 11 N·m | 97 lb in
Timing Belt Tensioner Bolt | 25 N·m | 18 lb ft
Timing Belt Tensioner Stud | 11 N·m | 97 lb in
Torque Rod Bracket Bolts | 55 N·m | 41 lb ft
Torque Rod-to-Frame Through Bolt | 55 N·m | 41 lb ft
Torque Rod-to-Torque Rod Brace Bolt | 55 N·m | 41 lb ft
Torque Rod-to-Torque Rod Bracket Through Bolt and Nut | 55 N·m | 41 lb ft
Upper Generator Adjustment Bolt | 23 N·m | 17 lb ft
Upper Rear Mounting Bracket Retaining Nuts | 55 N·m | 41 lb ft