For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .
3. Disconnect the speedometer cable (1) by pushing on the plastic tab.
4. Remove the 4 screws.
5. Disconnect the 3 electrical connectors.
6. Remove the instrument cluster (3).

### Installation Procedure

1. Connect the 3 instrument cluster electrical connectors.
2. Install the instrument cluster (3) to the instrument panel. Secure the cluster with the 4 screws.
3. Connect the speedometer cable (1).
4. Install the instrument cluster bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .
5. Connect the negative battery cable.