For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Interior Lights System Check? | -- | Go to Step 2 | Go to Interior Lamps System Check .
2 | Backprobe the dome lamp connector using J 35616-200 from cavity 2 to ground. Does the test lamp light? | -- | Go to Step 3 | Go to Step 4
3 | Replace the dome lamp assembly. Refer to Dome Lamp Replacement . Is the repair complete? | -- | Go to Interior Lamps System Check . | --
4 | Inspect for an open in the WHT wire between the junction block and the dome lamp. Is the connection OK? | -- | Go to Step 5 | Go to Step 6
5 | Replace the junction block. Is the repair complete? | -- | Go to Interior Lamps System Check . | --
6 | Repair the open in the WHT wire between the junction block and the dome lamp. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Interior Lamps System Check . | --