For 1990-2009 cars

## Front Side Door Jamb Switch Replacement 2 Door

### Removal Procedure

1. Remove the rubber boot (2) from the door-jamb switch (1).
2. Remove the screw which secures the switch (1) to the door jamb.
3. Perform the following steps in order to attain access to the electrical connector of the switch (1):

3.1. | Remove the lower quarter trim finish panel. Refer to Body Side Rear Trim Panel Replacement in Interior Trim.

3.2. | Remove the rear radio speaker. Refer to Radio Rear Speaker Replacement in Entertainment.

4. Disconnect the door-jamb switch electrical connector.
5. Remove the switch (1) from the vehicle.

### Installation Procedure

1. Connect the door-jamb switch electrical connector.
2. Install the door-jamb switch (1) to the vehicle. Secure the switch with the screw.
3. Perform the following steps:

3.1. | Install the rear radio speaker. Refer to Radio Rear Speaker Replacement in Entertainment.

3.2. | Install the lower quarter trim finish panel. Refer to Body Side Rear Trim Panel Replacement in Interior Trim.

4. Install the rubber boot (2) to the switch (1).

## Front Side Door Jamb Switch Replacement 4 Door

### Removal Procedure

1. Remove the rubber boot (2) from the door-jamb switch (1).
2. Remove the screw which secures the switch (1) to the door jamb.
3. Remove the lower center pillar trim panel in order to attain access to the electrical connector of the switch (1).
4. Disconnect the door-jamb switch electrical connector.
5. Remove the switch (1) from the vehicle.

### Installation Procedure

1. Connect the door-jamb switch electrical connector.
2. Install the door-jamb switch (1) to the vehicle. Secure the switch with the screw.
3. Install the lower center pillar trim panel to the vehicle.
4. Install the rubber boot (2) to the switch (1).