For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the system check? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 |

1. Turn the ignition switch to the ON position.
2. Backprobe the front wiper motor connector with a test lamp from cavity 5 to ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Test for an open in the BLU/WHT wire between the front wiper motor and combination switch. Was an open found? | -- | Go to Step 7 | Go to Step 5
4 | Test for an open in the YEL/BLU wire between the junction block and front wiper motor. Was an open found? | -- | Go to Step 7 | Go to Step 6
5 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in SIR. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
6 | Replace the wiper motor. Refer to Windshield Wiper Motor Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --
7 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --