For 1990-2009 cars

Inspect for the following conditions:

• | An overfilled reservoir

• | Air bubbles in the fluid

• | Loose pipe/hose connections

Perform the following actions when the steering gear and pump requires service:

• | Clean the leakage area upon disassembly.

• | Replace the locking seal.

• | Inspect the component sealing surfaces for damage.

• | Reset the fittings to the proper tightening specifications where required. Refer to Fastener Tightening Specifications .

The following complaints about the power steering system may be reported:

• | Fluid leakage on the garage floor

• | Visible fluid leaks on the steering gear or pump

• | Growling noise, especially when parking or when the engine is cold

• | The loss of power steering when parking

• | Heavy steering effort

When you troubleshoot these kinds of complaints, inspect for an external leak in the power steering system.