For 1990-2009 cars

### Removal Procedure

1. Gently pry off the outside rearview mirror garnish (8).
2. Remove the following components from the front door:

2.1. | The 3 screws

2.2. | The outside rearview mirror (7)

2.3. | The mirror gaskets, if necessary

### Installation Procedure

1. Install the mirror gaskets to the outside rearview mirror, if necessary.
2. Install the outside rearview mirror (7) to the front door. Secure the mirror with the 3 screws.
3. Install the outside rearview mirror garnish (8) to the door.