For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor to Bracket Bolts | 22.5-27.4 N·m | 16.5-20.1 lb ft
Belt Tension Pulley Nut | 45 N·m | 33 lb ft
Cylinder Pipe Assembly Nut C | 27 N·m | 19.5 lb ft
Cylinder Pipe Assembly Nut D | 17 N·m | 12.5 lb ft
High Pressure Hose Retaining Bracket Bolt | 10 N·m | 89 lb in
High Pressure Hose to High Pressure Pipe Flare Nut | 40 N·m | 30 lb ft
High Pressure Line Connector | 60 N·m | 44 lb ft
High Pressure Line to Pump Nut | 25 N·m | 18 lb ft
Inlet and Outlet Pipes | 40 N·m | 28.5 lb ft
Inlet Pipe Bolts | 8 N·m | 71 lb in
Power Steering Pump Mounting Bracket to Engine Bolts | 46.8-50.4 N·m | 63.7-68.6 lb ft
Power Steering Pump to Bracket Bolts | 35 N·m | 25 lb ft
Pressure Sensor | 18 N·m | 13 lb ft
Pump Cover Bolts | 24 N·m | 17.5 lb ft
Steering Gear Mounting Bracket Bolts | 25 N·m | 18 lb ft
Tie Rod End Castle Nuts | 43 N·m | 32 lb ft
Tie Rod to Power Steering Gear Ball Nut | 55 N·m | 40 lb ft
Upper and Lower Steering Shaft Joint Bolts | 25 N·m | 18 lb ft