For 1990-2009 cars

## Radio Rear Speaker Replacement Notchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear window shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement.
3. Disconnect the electrical connector.
4. Remove the screws and the rear speakers.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear speakers with the screws and tighten to 3 N·m (27 lb in).
2. Connect the electrical connector.
3. Install the rear window shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement.
4. Connect the negative battery cable.

## Radio Rear Speaker Replacement Hatchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear cargo area side trim panel. Refer to Cargo Area Side Trim Panel Replacement.
3. Disconnect the electrical connector.
4. Remove the screws and the rear speaker.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear speaker with the screws and tighten to 3 N·m (27 lb in).
2. Connect the electrical connector.
3. Install the rear cargo area side trim panel. Refer to Cargo Area Side Trim Panel Replacement.
4. Connect the negative battery cable.