For 1990-2009 cars

### Removal Procedure

1. Remove the seats and carpet.
2. Remove all trim panels.
3. Peel off the damaged deadener with a steel spatula, carefully remove deadener.

### Installation Procedure

1. Before applying the deadener, thoroughly clean and dry the areas to be applied.

Important: Avoid the parts mounting holes and service holes.

2. Note the areas on the panels to apply the deadener.
3. Heat the surface of deadener with a torch or heating gun until it adheres itself.

Important: Be careful not to burn the composite parts when heating.

Important: In order to take full advantage of the deadener, its face must adhere and contact the panels perfectly.

4. Push and adhere to the panel with a rubber spatula.
5. Install all trim panels.
6. Install seats and carpet.